# Template file for 'libcec'
pkgname=libcec
version=2.1.1
revision=1
wrksrc="${pkgname}-${pkgname}-${version}"
short_desc="USB CEC Adapter communication Library"
maintainer="Juan RP <xtraeme@gmail.com>"
homepage="https://github.com/Pulse-Eight/libcec"
license="GPL-2"
distfiles="https://github.com/Pulse-Eight/libcec/archive/libcec-${version}.tar.gz"
checksum=f61378798d900d496ed3a5ff7747b0bb35bdfec9b5c4168dcea38396e3569bf1

hostmakedepends="automake pkg-config libtool"
makedepends="libudev-devel lockdev-devel"

if [ "$XBPS_TARGET_MACHINE" = "armv6l" ]; then
	makedepends+=" rpi-firmware"
fi

pre_configure() {
	autoreconf -fi
}

do_configure() {
	if [ "$XBPS_TARGET_MACHINE" = "armv6l" ]; then
		configure_args+=" --enable-rpi "
		if [ "$XBPS_CROSS_BASE" ]; then
			configure_args+=" --with-rpi-include-path=${XBPS_CROSS_BASE}/opt/vc/include "
			configure_args+=" --with-rpi-lib-path=${XBPS_CROSS_BASE}/opt/vc/lib "
		else
			configure_args+=" --with-rpi-include-path=/opt/vc/include "
			configure_args+=" --with-rpi-lib-path=/opt/vc/lib "
		fi
	fi
	./configure ${configure_args} LDFLAGS=
}

do_build() {
	make ${make_build_args}
}

do_install() {
	make DESTDIR=${DESTDIR} install
}

cec-client_package() {
	depends="libcec>=${version}"
	short_desc="${short_desc} -- client tool"
	pkg_install() {
		vmove usr/bin
	}
}

libcec_package() {
	pkg_install() {
		vmove usr
	}
}
